

**LAB SESSION # 06**


* **3\*8 DECODER CIRCUIT :**




* **WHEN ALL THE ENABLE PINS ARE CONNECTED TO VCC:**



* **WHEN ALL THE ENABLE PINS ARE CONNECTED TO GROUND:**



* **CASCADING TWO 2\*4 DECODER TO 3\*8 DECODER:**



* **Prepared by Muhammad Faraz Ansar (SE-061)**